For 1990-2009 cars

• | Inspect for a lack of lubrication in ball joints, drive axle joints and tie rod ends.

• | Inspect for damaged suspension components.

• | Inspect for worn control arm bushings or tie rod ends.

• | Inspect for a loose stabilizer shaft.

• | Inspect for loose wheel nuts.

• | Inspect for loose suspension bolts.

• | Inspect the wheel covers.

• | Inspect the bearing rack preload.

• | Inspect for a worn strut dampener or mountings.

• | Inspect for a improperly positioned spring.