For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
DEFINITION: Lubricant leaks from around the clutch area
1 |

1. Disassemble the input shaft. Refer to Input Shaft Disassemble
2. Check the components on the input shaft for wear or damage:

• | The bearing seal

• | The seal mating surfaces

• | The rollers

Are any of the components worn or damaged?

Go to Step 2

Refer to Fluid Leak Diagnosis and Repair

2 | Service, repair, or replace any worn or damaged components. Refer to Input Shaft Assemble Did the leak stop? |  | System OK | Refer to Fluid Leak Diagnosis and Repair