For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 |

1. Disassemble the transaxle case. Refer to Unit Repair.
2. Check the following components for wear or damage.

• | The 1st speed constant-mesh gears

• | The 1st/2nd synchronizer

Are any of the components worn, chipped, or scored?

--

Go to Step 2

Go to Bearing Noise

2 | Service, repair, or replace the components as necessary. Refer to Unit Repair. Did the noise disappear? | -- | System OK | Go to Bearing Noise