For 1990-2009 cars

### Removal Procedure

1. Remove the forward servo attaching bolts.
2. Remove the servo cover.
3. Remove the servo piston assembly.
4. Remove the following items:

• | Sealing ring

• | Servo spring

5. For disassembly of the forward servo piston assembly, refer to Forward Servo Disassemble .

### Installation Procedure

1. Install the following items:

• | Servo spring

• | Sealing ring

2. Install the servo piston assembly.
3. Install the servo cover.
4. Install the forward servo attaching bolts.
5. For disassembly of the servo piston assembly, refer to Transmission Unit Repair Manual.