For 1990-2009 cars

### Removal Procedure

#### Tools Required

• | J 1859-A Steering Wheel Puller

• | J 42578 Steering Wheel Puller

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Disable the supplemental inflatable restraint (SIR) system. Refer to Disabling the SIR System in SIR.
3. Remove the inflator module. Refer to Inflatable Restraint Steering Wheel Module Replacement in SIR.
4. Remove the steering wheel nut (1).
5. Remove the steering wheel using the J 1859-A and J 42578
6. Disconnect the electrical connectors (4) from the column.
7. Route the electrical connectors (4) through the steering wheel opening.
8. Remove the steering wheel (2) from the vehicle.

### Installation Procedure

1. Route the electrical connectors (4) through the steering wheel opening.
2. Connect the electrical connector (4) to the steering column (3).
3. Install the steering wheel on the steering column (3).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the steering wheel nut (1) on the steering column (3).

Tighten
Tighten the nut to 40 N·m (29 lb ft).

5. Install the inflator module. Refer to Inflatable Restraint Steering Wheel Module Replacement in SIR.
6. Enable the SIR system. Refer to Enabling the SIR System in SIR.
7. Connect the negative battery cable.