For 1990-2009 cars

### Removal Procedure

1. Remove starter from vehicle. Refer to Starter Motor Replacement Starter Motor Replacement .
2. Disconnect the field lead.
3. Remove the solenoid to drive housing attaching screws and remove the solenoid by twisting.

### Installation Procedure

1. Twist the solenoid into position and install the attaching screws.
2. Install the field strap.
3. Install starter to engine. Refer to Starter Motor Replacement Starter Motor Replacement .