For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to

   Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

   in General Information.
2. Raise the vehicle. Support the vehicle. Refer to General Vehicle Lifting and Jacking in General Information.
3. Remove the case side cover. Refer to Case Side Cover Replacement (W/ Gasket) .
4. Remove the 1-2 shift solenoid retainer.
5. Remove the 1-2 shift solenoid.
6. Remove the PWM solenoid retainer.
7. Remove the PWM solenoid.
8. Remove the TCC solenoid retainer.
9. Remove the TCC solenoid.
10. Remove the 3-4 shift solenoid retainer.
11. Remove the 3-4 shift solenoid.

### Installation Procedure

1. Install the 3-4 shift solenoid.
2. Install the 3-4 shift solenoid retainer.
3. Install the TCC solenoid.
4. Install the TCC solenoid retainer.
5. Install the PWM solenoid.
6. Install the PWM solenoid retainer.
7. Install the 1-2 shift solenoid.
8. Install the 1-2 shift solenoid retainer.
9. Install the case side cover, new gaskets and attaching bolts. Refer to Case Side Cover Replacement (W/ Gasket) .
10. Connect the negative battery cable.
11. Lower the vehicle.
12. Adjust the fluid level.