For 1990-2009 cars

### Removal Procedure

1. Run the wiper arms to the mid-wipe position.
2. Lift the blade retaining latch.
3. Remove the wiper blade from the arm.

### Installation Procedure

Important:

• | Use only 19-inch beam-type wiper blades.

• | The wiper blades must be installed with the blade retaining latch pointed inward towards the wiper arm side of the mounting pin.

1. Install the blade onto the arm.
2. Park the wipers if they are at the mid-wipe position.