For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Drums
Inside Diameter | 200.00-200.40 mm | 7.874-7.890 in
Runout | 0.15 mm | 0.006 in
Maximum Re-bore Diameter | 200.64 mm | 7.899 in
Discard Diameter | 201.40 mm | 7.929 in
Brake Pedal Travel (see note*) | 63.5 mm | 2.5 in
Brake Rotors
Rotor Diameter | 259 mm | 10.197 in
Lateral Runout | 0.08 mm | 0.003 in
Thickness Variation | 0.013 mm | 0.0005 in
Rotor Thickness | 20.48 mm | 0.806 in
Minimum Thickness After Refinish | 19.08 mm | 0.751 in
Discard Thickness | 18.70 mm | 0.736 in
Caliper Bore Diameter | 57 mm | 2.244 in
Master Cylinder Bore Diameter | 22.20 mm | 0.874 in
Wheel Cylinder Bore Diameter | 17.5 mm | 0.689 in

*Note: Brake pedal travel maximum with 445 N (100 lb) force applied to pedal with ignition OFF and vacuum assist deleted

All brake drums and rotors have a discard dimension cast into them. This is a wear dimension and not a refinish dimension. Any drum or rotor which does not meet the specification should be replaced.