For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Power Window System Check? | -- | Go to Step 2 | Go to Power Windows System Check
2 |

1. Disconnect the right rear window switch connector.
2. Turn the ignition switch to the RUN position.
3. Connect a test lamp between connector terminal A and terminal E.
4. Operate the window switch to the UP and the DOWN positions.

Does the test lamp light in both of the positions?

--

Go to Step 3

Go to Step 5

3 |

1. Connect a fused jumper between the connector terminal A and terminal D.
2. Connect a fused jumper between the connector terminal E and terminal H.
3. Operate right rear window switch on the master switch to the UP and to the DOWN positions.

Does the rear window operate?

--

Go to Step 4

Go to Step 6

4 | Replace the right rear window switch. Refer to Rear Side Door Window Switch Replacement . Is the repair complete? | -- | Go to Power Windows System Check | --
5 | Test for an open in CKT 170 and CKT 171. Did you find an open in either of the circuits? | -- | Go to Step 7 | Go to Step 8
6 | Test for an open in CKT 670 and CKT 671. Did you find an open in either of the circuits? | -- | Go to Step 7 | Go to Step 9
7 | Repair the faulty circuit. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --
8 | Replace the master switch assembly. Refer to the following procedures:

• | Door Lock and Side Window Switch Replacement

• | Door Lock and Side Window Switch Replacement

• | Door Lock and Side Window Switch Replacement

Is the repair complete?

--

Go to Power Windows System Check

--

9 | Replace the right rear window motor. Refer to the following procedures:

• | Door Window Regulator Motor Replacement

• | Door Window Regulator Motor Replacement

Is the repair complete?

--

Go to Power Windows System Check

--