For 1990-2009 cars

1. Inspect the forward band assembly (688) for the following conditions:

• | Damaged or severely worn friction material

• | Damaged apply or anchor pin features

2. Inspect the thrust washer (691) from the differential carrier internal gear for damage.
3. Position the transmission case so that the flange for the case cover is facing up.
4. Install the thrust washer (691) for the differential carrier internal gear into the case. Position as indicated.
5. Install the forward band assembly (688) into the case.

• | Locate the band assembly onto the forward band anchor pin

• | Position the band apply pin feature in the opening of the case