For 1990-2009 cars

# RETENTION OF FROM DOOR LOCK SWITCH (RPL. DOOR LOCK BEZEL)

#### SUBJECT: RETENTION OF FRONT DOOR LOCK SWITCH (REPLACE DOOR LOCK BEZEL)

VEHICLES AFFECTED: 1992-93 OLDSMOBILE "N" MODELS

THIS BULLETIN SUPERSEDES AND REPLACES CORPORATE BULLETIN REFERENCE NUMBER 331012.- THIS BULLETIN IS BEING REVISED TO INCLUDE THE 1992 MODEL YEAR

#### CONDITION:

Some owner's of 1992 and 1993 Oldsmobile "n" vehicles (built before VIN breakpoint PM016842) equipped with power door locks may comment on the front left and/or fight-hank lock switch assemblies becoming disengaged from the bezel when the switch is pressed.

#### CAUSE:

Lock switch retention legs on the switch bezel are too flexible to maintain pressure against lock switch when force is applied.

#### CORRECTION:

Replace door lock bezel with P/N 22588802 (RH) or 22588803 (LH) using the service procedure found in Section 10-6 of the 1993 service manual.

For vehicles repaired under warranty use:

Labour Time: 0.2 Hours

#### BULLETIN REFERENCES:

Corporate Ref. 331012

General Motor's of Canada 93-10-182 Oldsmobile Division 93-T-53

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.