For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Check for mismatched or uneven tire pressure. Is the tire pressure mismatched or uneven? | -- | Go to Tire Repair | Go to Step 2
2 | Check for proper lubrication in the ball joints and the tie rod ends. Do the ball joints and the tie rod ends lack lubrication? | -- | Go to Stabilizer Shaft Replacement | Go to Step 3
3 | Check the condition of the strut dampeners. Are the strut dampeners worn? | -- | Go to Strut Assembly Replacement | Go to Step 4
4 | Check for proper tightness of the stabilizer shaft. Is the stabilizer shaft loose? | -- | Go to Stabilizer Shaft Replacement | Go to Step 5
5 | Check for broken or sagging springs. Are the springs broken or sagging? | -- | Go to Spring Replacement in Front Suspension | Go to Step 6
6 | Check for proper preload of the rack bearing. Is the rack bearing preload appropriate? | -- | Go to Step 7 | Go to Steering in Steering, Suspension, Tires and Wheel Diagnosis
7 | Check the condition of the hub and bearing assembly. Is the hub an bearing assembly worn? | -- | Go to Front Wheel Bearing and Hub Replacement | Go to Step 8
8 | Check for proper alignment of the front-wheel or the rear-wheel. Is the front-wheel or the rear-wheel misaligned? | -- | Go to Wheel Alignment Specifications | System OK