For 1990-2009 cars

## Valve Rocker Arm Cover Removal Left Side

### Left Valve Rocker Cover Removal

1. Remove the thermostat bypass hose clamp.
2. Remove the thermostat coolant bypass pipe retaining bolt, nut, and screw.
3. Remove the thermostat coolant bypass pipe.
4. Remove the valve rocker cover bolts.
5. Remove the valve rocker cover.
6. Remove the valve rocker gasket.

## Valve Rocker Arm Cover Removal Right Side

1. Remove the generator bracket bolts.
2. Remove the generator bracket assembly.
3. Remove the valve rocker cover bolts.
4. Remove the valve rocker cover.
5. Remove the valve rocker gasket.