For 1990-2009 cars

# SMU - SEC. 3C-3 - REV. TORQUE SPECS FOR CONTROL ARM TO

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 3C-3 - REVISED TORQUE SPECIFICATIONS FOR CONTROL ARM TO CROSSMEMBER BOLTS

#### MODELS: 1998 CHEVROLET MALIBU 1998 OLDSMOBILE CUTLASS

THIS BULLETIN IS BEING ISSUED TO REVISE THE TORQUE SPECIFICATIONS FOR THE CONTROL ARM TO CROSSMEMBER BOLTS (FRONT BUSHING) AND CONTROL ARM TO CROSSMEMBER BOLTS (REAR VERTICAL BUSHING) AS SHOWN IN THE 1998 SERVICE MANUAL, SECTION 3C, PAGE 3-31 FOR FRONT SUSPENSION.

THE CORRECT TORQUE SPECIFICATION SHOULD BE AS FOLLOWS:

TIGHTEN

* TIGHTEN THE CONTROL ARM TO THE CROSSMEMBER BOLTS (FRONT BUSHING) TO 60 N.M (44 LB FT) PLUS 120 DEGREES ROTATION.

* TIGHTEN THE CONTROL ARM TO THE CROSSMEMBER BOLTS (REAR VERTICAL BUSHING) TO 100 N.M (74 LB FT) PLUS 180 DEGREES ROTATION.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1998 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.