For 1990-2009 cars

## DTC P0719 Brake Switch Circuit Low Input 3.1L VIN M

Handling ESD Sensitive Parts Notice
OBD II Symbol Description Notice
Automatic Transmission Controls Schematics 3.1L VIN M
Automatic Transmission Components 3.1L VIN M

### Circuit Description

The Torque Converter Clutch (TCC) brake switch reports brake pedal status to the Powertrain Control Module (PCM). The brake switch indicates that the brake pedal is either applied or released. The normally-closed switch supplies battery voltage on circuit 420 to the PCM. Applying the brake pedal opens the brake switch, interrupting voltage to the PCM. When the PCM receives 0 volts at the brake switch input, the PCM turns OFF the TCC Solenoid Valve.

If the PCM detects an open brake switch (stuck ON) during acceleration, then DTC P0719 sets. DTC P0719 is a type D DTC.

### Conditions for Setting the DTC

• | No VSS DTCs P0502 or P0503.

• | The vehicle speed is less than 8 km/h (5 mph).

• | Accelerate the vehicle to 32 km/h (20 mph) taking 4 seconds.

• | The vehicle speed remains above 32 km/h (20 mph) for 6 seconds.

• | The above conditions must occur 7 times with the brake switch ON for more than 15 minutes, and the PCM receiving no voltage input for 2 seconds.

### Action Taken When the DTC Sets

• | The PCM requires a throttle angle greater than 6% and a vehicle speed greater than 71 km/h (44 mph) in order to apply the TCC.

• | Disregard the brake switch for TCC control if the following four conditions are true:

- | The TP angle was formerly greater than 12%.

- | The vehicle speed was formerly greater than 75 km/h (47 mph).

- | The TP angle is now greater than 6%.

- | The vehicle speed is now greater than 70 km/h (44 mph).

• | The PCM does not illuminate the Malfunction Indicator Lamp (MIL).

### Conditions for Clearing the DTC

• | A scan tool can clear the DTC from the PCM history. The PCM clears the DTC from the PCM history if the vehicle completes 40 warm-up cycles without a failure reported.

• | The PCM cancels the DTC default actions when the fault no longer exists and the ignition is OFF long enough in order to power down the PCM.

### Diagnostic Aids

• | Ensure that the TCC brake switch is properly adjusted.

• | Check the PCM calibration for a current update.

• | Inspect the wiring for poor electrical connections at the PCM. Inspect the wiring at the transmission 7-way connector. Look for the following conditions:

- | A bent terminal

- | A backed out terminal

- | A damaged terminal

- | Poor terminal tension

- | A chafed wire

- | A broken wire inside the insulation

• | When diagnosing for an intermittent short or open condition, massage the wiring harness while watching the test equipment for a change.

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. If DTCs P0740, P0753, and P0758 are also set, then the TCC fuse is open.

2. This step isolates the fault between the TCC Brake Switch and the harness.

#### DTC P0719 TCC Brake Switch Circuit Low

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Powertrain On-Board Diagnostic (OBD) System Check performed? | -- | Go to Step 2 | Go to Powertrain On Board Diagnostic (OBD) System Check
2 |

1. Install the scan tool.
2. With the engine OFF, turn the ignition switch to the RUN position.

Important: Before clearing the DTCs, use the scan tool in order to record the Failure Records for reference. The Clear Info function will erase the data.

3. Record the DTC Failure Records.
4. Inspect the Alarm fuse for an open.

Did you find and correct a problem?

--

Go to Step 3

Go to Step 4

3 |

1. Inspect circuits 39 and 420 for a short to ground.
2. Repair circuits 39 and 420 if necessary.

Refer to Troubleshooting Procedures, Section 8.

Did you find and correct a problem?

--

Go to Step 8

--

4 |

1. Select Brake Switch on the scan tool.
2. Disconnect the TCC brake switch.
3. Install a fused jumper from terminal C to terminal D of the brake switch connector.

Does the brake status change from Open to Closed?

--

Go to Step 5

Go to Step 6

5 | Replace the TCC brake switch. Refer to Brake Switch Replacement, Section 5. Is the replacement complete? | -- | Go to Step 8 | --
6 |

1. Inspect circuits 420 and 39 for an open.
2. Repair circuits 420 or 39 if necessary.

Refer to Troubleshooting Procedures, Section 8.

Did you find and correct a problem?

--

Go to Step 8

Go to Step 7

7 | Replace the PCM. Refer to Powertrain Control Module Replacement/Programming , Section 6 Is the replacement complete? | -- | Go to Step 8 | --
8 | In order to verify your repair, perform the following procedure:

1. Select DTC.
2. Select Clear Info.
3. Operate the vehicle under the following conditions:

• | Turn the ignition switch to the RUN position.

• | The TCC brake switch must be OFF for more than 2 seconds.

4. Select Specific DTC. Enter DTC P0719.

Has the test run and passed?

--

System OK

Begin the diagnosis again. Go to Step 1

## DTC P0719 Brake Switch Circuit Low Input 2.4L VIN T

Handling ESD Sensitive Parts Notice
OBD II Symbol Description Notice
Automatic Transmission Controls Schematics 2.4L VIN T
Automatic Transmission Components 2.4L VIN T

### Circuit Description

The Torque Converter Clutch (TCC) brake switch reports brake pedal status to the Powertrain Control Module (PCM). The brake switch indicates that the brake pedal is either applied or released. The normally-closed switch supplies battery voltage on circuit 420 to the PCM. Applying the brake pedal opens the brake switch, interrupting voltage to the PCM. When the PCM receives 0 volts at the brake switch input, the PCM turns OFF the TCC Solenoid Valve.

If the PCM detects an open brake switch (stuck ON) during acceleration, then DTC P0719 sets. DTC P0719 is a type D DTC.

### Conditions for Setting the DTC

• | No VSS DTC P0502 or P0503

• | The vehicle speed is less than 8 km/h (5 mph).

• | Accelerate the vehicle to 32 km/h (20 mph) taking 4 seconds.

• | The vehicle speed remains above 32 km/h (20 mph) for 6 seconds.

• | The above conditions must occur 7 times with the brake switch ON for more than 15 minutes, and the PCM receiving no voltage input for 2 seconds.

### Action Taken When the DTC Sets

• | Disregard the brake switch for TCC scheduling if all of the following conditions are met:

- | The throttle position is greater than 6%.

- | The vehicle speed is greater than 70 km/h (44 mph).

- | The throttle position was previously greater than 12%, while the vehicle speed was greater than 72 km/h (47 mph).

- | The brake switch has not been OFF for more than 2 seconds in this ignition cycle.

• | The PCM does not illuminate the Malfunction Indicator Lamp (MIL).

### Conditions for Clearing the DTC

• | A scan tool can clear the DTC from the PCM history. The PCM clears the DTC from the PCM history if the vehicle completes 40 warm-up cycles without a failure reported.

• | The PCM cancels the DTC default actions when the fault no longer exists and the ignition is OFF long enough in order to power down the PCM.

### Diagnostic Aids

• | Ensure that the TCC brake switch is properly adjusted.

• | Check the PCM calibration for a current update.

• | Inspect the wiring for poor electrical connections at the PCM. Inspect the wiring at the transmission 7-way connector. Look for the following conditions:

- | A bent terminal

- | A backed out terminal

- | A damaged terminal

- | Poor terminal tension

- | A chafed wire

- | A broken wire inside the insulation

• | When diagnosing for an intermittent short or open condition, massage the wiring harness while watching the test equipment for a change.

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. This step ensures that DTC P0719 failure records were recorded.

2. This step isolates the fault between the TCC Brake Switch and the harness.

#### DTC P0719 TCC Brake Switch Circuit Low

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Powertrain On-Board Diagnostic (OBD) System Check performed? | -- | Go to Step 2 | Go to Powertrain On Board Diagnostic (OBD) System Check
2 |

1. Install the scan tool.
2. With the engine OFF, turn the ignition switch to the RUN position.

Important: Before clearing the DTCs, use the scan tool in order to record the Failure Records for reference. The Clear Info function will erase the data.

3. Record the DTC Failure Records.
4. Inspect the Alarm fuse for an open.

Did you find and correct a problem?

--

Go to Step 3

Go to Step 4

3 |

1. Inspect circuits 39 and 420 for a short to ground.
2. Repair circuits 39 and 420 if necessary.

Refer to Troubleshooting Procedures, Section 8.

Did you find and correct a problem?

--

Go to Step 8

--

4 |

1. Select Brake Switch on the scan tool.
2. Disconnect the TCC brake switch.
3. Install a fused jumper from terminal A to terminal B of the brake switch connector.

Does the brake status change from Open to Closed?

--

Go to Step 5

Go to Step 6

5 | Replace the TCC brake switch. Refer to Brake Switch Replacement, Section 5. Is the replacement complete? | -- | Go to Step 8 | --
6 |

1. Inspect circuit 39 and circuit 420 for an open.
2. Repair the circuits, if necessary.

Refer to Troubleshooting Procedures, Section 8.

Did you find and correct a problem?

--

Go to Step 8

Go to Step 7

7 | Replace the PCM. Refer to Powertrain Control Module/EEPROM Replacement/Programming , Section 6 Is the replacement complete? | -- | Go to Step 8 | --
8 | In order to verify your repair, perform the following procedure:

1. Select DTC.
2. Select Clear Info.
3. Operate the vehicle under the following conditions:

• | Turn the ignition switch to the RUN position.

• | The TCC brake switch must be OFF for more than 2 seconds.

4. Select Specific DTC. Enter DTC P0719.

Has the test run and passed?

--

System OK

Begin the diagnosis again. Go to Step 1