For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to

   Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

   in General Information.
2. Disconnect the clutch actuator cylinder line.
3. Remove the transmission. Refer to Transmission Replacement in Manual Transmission.
4. Remove the clutch actuator cylinder from the transmission.

### Installation Procedure

1. Lubricate the inside diameter of the bearing with GM P/N 12345777, or equivalent.
2. Install the clutch actuator cylinder to the transmission.
3. Install the transmission. Refer to Transmission Replacement in Manual Transmission.
4. Connect the clutch actuator cylinder line.
5. Bleed the hydraulic system. Refer to Hydraulic Clutch Bleeding .
6. Connect the negative battery cable.