For 1990-2009 cars

# J38715 SIR DRIVER/PASSENGER LOAD TOOL AND ADAPTER

#### SUBJECT: INFORMATION ON J38715 SIR DRIVER/PASSENGER LOAD TOOL AND ADAPTER J38715-5

#### MODELS: 1993 CHEVROLET CAMARO 1993 PONTIAC FIREBIRD AND BONNEVILLE 1993 BUICK PARK AVENUE 1994 PASSENGER CARS AND U-VANS (EXCEPT CHEVROLET CAVALIER, GEO AND PONTIAC SUNBIRD AND LEMANS)

THIS BULLETIN CANCELS AND REPLACES GM SERVICE BULLETIN NO. 316109, WHICH WAS PUBLISHED WITH A GROUP REFERENCE OF ENGINE. PLEASE DISCARD BULLETIN 316109.

THIS BULLETIN ADVISES USE OF THE J38715 SIR DRIVER/PASSENGER LOAD TOOL FOR SUBSTITUTION OF THE DRIVER INFLATOR MODULE. WHEN CONNECTING THE LOAD TOOL TO THE LEAD FROM THE SIR COIL WHICH CONNECTS TO THE DRIVER INFLATOR MODULE, ADAPTER J38715-5 MUST BE USED ON THE LOAD TOOL LEAD LABELED "STEERING WHEEL".

FIGURES: 1

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.