For 1990-2009 cars

Table 1: | Horizontal Operation of the Seat Not Smooth (Jerky) Hard Operation
Table 2: | Horizontal Chuck or Looseness

#### Horizontal Operation of the Seat Not Smooth (Jerky) Hard Operation

Problem | Action
--- | ---
Improper lubrication of the adjuster shoes and the channels. | Lubricate the adjuster's upper channel and the plastic shoes.
The adjuster horizontal actuator gear is too tight to rack the gear. | Refer to Seat Adjuster Horizontal Actuator Adjustment .

#### Horizontal Chuck or Looseness

Problem | Action
--- | ---
The horizontal actuator is improperly adjusted to rack the gear. | Refer to Seat Adjuster Horizontal Actuator Adjustment .