For 1990-2009 cars

### Removal Procedure

1. Raise the hood.
2. Install protective covering over the fenders in order to prevent damage to the paint.
3. Remove the wiper arms and the blade assemblies.
4. Remove the screws (1) from the air inlet screen.
5. Remove the air inlet screen (2).

### Installation Procedure

1. Install the air inlet screen (2).
2. Install the screws (1) to the air inlet screen.
3. Install the wiper arms and the blade assemblies.