For 1990-2009 cars

Notice: Do not allow the bearings to spin. Turn the bearings slowly by hand. Spinning bearings may cause damage to the rollers.

Inspect the thrust washers for wear or damage. Replace worn or damaged thrust washers.

Inspect the condition of all needle bearings, roller bearings and thrust bearings. Wash the bearings thoroughly in a cleaning solvent. Apply compressed air to the bearings.

Lubricate the bearings with a light oil. Check the bearings for roughness by slowly turning the race by hand.