For 1990-2009 cars

(1) | Ignition Coil Assembly
(2) | Cylinder #1
(3) | Cylinder #4
(4) | Cylinder #6
(5) | Cylinder #3
(6) | Cylinder #2
(7) | Cylinder #5
(8) | Harness Assembly Clip
(9) | Left Hand Harness Assembly
(10) | Harness Assembly Clip
(11) | Cylinder #6
(12) | Cylinder #4
(13) | Cylinder #2
(14) | Cylinder #5
(15) | Cylinder #3
(16) | Cylinder #1
(17) | Harness Assembly Clip
(18) | Right Hand Harness Assembly

When replacing spark plug cables (secondary wiring), route the cables correctly and thorough the proper retainer. Use care when unlocking retainers. Failure to route the cables properly can lead to radio ignition noise and cross-firing of the plugs, or shorting of the leads to ground. The silicone spark plug boots form a tight seal on the plug and the boot should be twisted 1/2 turn while removing.