For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Power Mirrors System Check? | -- | Go to Step 2 | Go to Outside Mirrors System Check
2 |

1. Disconnect the outside mirror switch connector.
2. Connect a test lamp between the connector terminal E and terminal D.

Does the test lamp light?

--

Go to Step 3

Go to Step 4

3 | Inspect the terminal connectors. Refer to Connector Repairs in Wiring Systems. Are the terminal connectors OK? | -- | Go to Step 6 | Go to Step 8
4 | Connect a test lamp between terminal E and ground. Does the test lamp light? | -- | Go to Step 5 | Go to Step 7
5 | Repair an open in CKT 150. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Outside Mirrors System Check | --
6 | Replace the outside mirror switch. Refer to Mirror Switch Replacement. Is the repair complete? | -- | Go to Outside Mirrors System Check | --
7 | Repair an open in CKT 1732. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Outside Mirrors System Check | --
8 | Repair the faulty connector. Refer to Connector Repairs in Wiring Systems. Is the repair complete? | -- | Go to Outside Mirrors System Check | --