For 1990-2009 cars

### Removal Procedure

1. Open the rear compartment lid.
2. Remove the 4 wing nuts in order to remove the lens assembly from the vehicle.
3. Turn the back-up lamp socket counter-clockwise in order to remove the socket from the lamp assembly.
4. Remove the back-up lamp bulb from the socket.

### Installation Procedure

1. Install the back-up lamp bulb to the socket.
2. Install the socket into the lamp assembly. Turn the socket clockwise in order to secure the socket.
3. Use the 4 wing nuts in order to install the lamp assembly to the vehicle.
4. Close the rear compartment lid.