For 1990-2009 cars

### Removal Procedure

1. Peel the auxiliary weather-strip from the windshield side reveal molding (1).
2. Remove the screws (2) from the windshield side reveal molding (1).
3. Remove the windshield side reveal molding (1) by sliding the molding downward and disengaging the molding from the windshield upper reveal molding (3).

### Installation Procedure

1. Install the windshield side reveal molding (1) by sliding the molding upward into the windshield upper reveal molding (3).
2. Install the screws (2) that retain the windshield side reveal molding.
3. Install the auxiliary weather-strip to the windshield side reveal molding.