For 1990-2009 cars

#### Fastener Tightening Specifications

Application | Specifications
--- | ---
Metric | English
Ball Joint Stud Nut | 55-65 N·m | 41-48 lb ft
Caliper to Knuckle Bolts | 51 N·m | 38 lb ft
Control Arm to Suspension Support Bolts (Front Bushing) | 60 N·m plus 90° rotation | 45 lb ft plus 90° rotation
Control Arm to Suspension Support Bolts (Rear Vertical Bushing) | 100 N·m | 74 lb ft
Wheel Drive Shaft Nut | 100 N·mplus 40° rotation | 74 lb ft plus 40° rotation
Hub and Bearing Assembly to Steering Knuckle Bolts | 95 N·m | 70 lb ft
Stabilizer Link | 30 N·m | 22 lb ft
Stabilizer Shaft Bushing to Control Arm Nuts | 21 N·m | 15 lb ft
Stabilizer Shaft to Suspension Support Nuts | 30 N·m | 22 lb ft
Steering Knuckle to Strut Assembly Nuts | 180 N·m | 133 lb ft
Strut Assembly to Body Bolt | 25 N·m | 19 lb ft
Strut Assembly to Body Nuts | 25 N·m | 19 lb ft
Strut Nut to Strut Rod | 70 N·m | 52 lb ft
Suspension Support Center Bolts | 120 N·m | 89 lb ft
Suspension Support Front Bolts | 120 N·m | 89 lb ft
Suspension Support Rear Bolts | 120 N·m | 89 lb ft
Tie Rod End to Strut Nut | 57 N·m | 42 lb ft