For 1990-2009 cars

### Removal Procedure

1. Remove the negative battery cable.
2. Note the position of the hoses for installation.
3. Remove the electrical connector and hoses from solenoid.
4. Release the lock tab on the solenoid mounting bracket.
5. Remove the solenoid.

### Installation Procedure

1. Bend tab on mounting bracket to retain the EVAP purge solenoid valve.
2. Install the solenoid to solenoid mounting bracket.

Once installed pull on the solenoid to ensure that the part will be held in place.

3. Install the electrical connector and hoses to solenoid.
4. Connect the negative battery cable.