For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 39500-B A/C Refrigerant Recover, Recharging, and Recycling Station

1. Recover the A/C system. Refer to Refrigerant Recovery and Recharging .
2. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
3. Remove the right tire/wheel assembly. Refer to Wheel Removal in Tires and Wheels.
4. Partially remove the right splash guard.
5. Remove the line (3) from the receiver dehydrator (4). Discard the O-ring (1) seals.
6. Remove the line from the condenser (2). Discard the O-ring (1) seals.

### Installation Procedure

#### Tools Required

J 39500-B A/C Refrigerant Recover, Recharging, and Recycling Station

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the line to the condenser (2) using new O-ring (1) seals.

Tighten
Tighten the fitting to 28 N·m (21 lb ft).

2. Install the line (3) to the receiver dehydrator (4) using new O-ring (1) seals.

Tighten
Tighten the fitting to 28 N·m (21 lb ft).

3. Install the right splash guard.
4. Install the right tire/wheel assembly. Refer to Wheel Installation in Tires and Wheels.
5. Lower the vehicle.
6. Evacuate and charge the A/C system. Refer to Refrigerant Recovery and Recharging .