For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 |

1. Disassemble the transaxle case. Refer to Unit Repair.
2. Check the following components for wear or damage.

• | The idler gear

• | The idler gear bushing

• | The input gear

• | The output gear

Are any of the components worn or damaged?

--

Go to Step 2.

Go to Transmission Replacement

2 | Service, repair, or replace the components as necessary. Refer to Unit Repair. Did the noise disappear? | -- | System OK | Go to Transmission Replacement