For 1990-2009 cars

1. Insert the transmission oil dam (27) into the case.
2. Insert the manual valve link and spring assembly into the manual shift shaft detent lever.
3. Pull back the manual valve spring (403) and connect the manual valve link (402) to the manual valve.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Attach the manual shift shaft detent assembly (804) to the case with a bolt (805).

Tighten
Tighten the bolt to 12 N·m (106 lb in).