For 1990-2009 cars

#### '97 4T60-E Component Resistance Chart (created for '97 Hcar)

Cavities | Component | Resistance @ 20°C (68°F) | Resistance @ 88°C (190°F)
--- | --- | --- | ---
A-E | 1-2 Shift Solenoid valve | 19-24ohms | 24-31ohms
B-E | 2-3 Shift Solenoid valve | 19-24ohms | 24-31ohms
C-E | Torque Converter Clutch (TCC) Pulse Width Modulation (PWM) Solenoid valve | 10-12ohms | 13-15ohms
D-E | Torque Converter Clutch (TCC) Solenoid valve | 19-24ohms | 24-31ohms
F-G | Automatic Transmission Fluid Temperature (TFT) Sensor | 3164-3867ohms | 225-285ohms