For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Wiper/Washer System Check? | -- | Go to Step 2 | Go to Wiper/Washer System Check or Wiper/Washer System Check
2 |

1. Disconnect the wiper motor connector C2.
2. Turn the ignition switch to RUN.
3. Turn the wiper switch to HIGH.
4. Connect a test lamp from connector C2, terminal A, to ground.

Does the test lamp light?

--

Go to Step 3

Go to Step 6

3 | Test for a poor connection at the wiper motor connector C2, terminal A. Does a poor connection exist? | -- | Go to Step 4 | Go to Step 5
4 | Repair the poor connection at the wiper motor connector C2, terminal A. Did you complete the repair? | -- | Go to Wiper/Washer System Check or Wiper/Washer System Check | --
5 | Replace the wiper motor. Refer to Windshield Wiper Motor Replacement . Did you complete the repair? | -- | Go to Wiper/Washer System Check or Wiper/Washer System Check | --
6 | Test for an open in CKT 92. Does an open exist? | -- | Go to Step 7 | Go to Step 8
7 | Repair the open in CKT 92. Did you complete the repair? | -- | Go to Wiper/Washer System Check or Wiper/Washer System Check | --
8 | Replace the wiper/washer switch. Refer to Windshield Wiper and Washer Switch Replacement - On Vehicle . Did you complete the repair? | -- | Go to Wiper/Washer System Check or Wiper/Washer System Check | --