For 1990-2009 cars

# RIGHT SIDE I/P AIR OUTLET OFF DOOR BLOWS CLOSED

#### SUBJECT: RIGHT SIDE INSTRUMENT PANEL AIR OUTLET SHUT-OFF DOOR BLOWS CLOSED (WRAP HUB OF RETAINER WITH TAPE)

#### VEHICLES AFFECTED: 1992 "N" MODELS

#### APPLICATION:

------------ 1992 Oldsmobile Achieva

#### CONDITION:

---------- Some owners of 1992 "N" Achieva models may comment that the right instrument panel air outlet shut-off door blows closed when in the MAX, NORM, BI-LEVEL, or VENT mode.

#### CAUSE:

----- Insufficient friction in the mechanism to hold the set position.

#### CORRECTION:

---------- 1. Remove air outlet from instrument panel, reference attachment. 2. Remove barrel assembly from air outlet housing. 3. Remove black retainer from thumb wheel. 4. Wrap the "hub" of the retainer with a 6mm x 6mm (1/4 inch x 1/4 inch) piece of electrical tape. 5. Reinstall the retainer onto the housing. 6. Check thumb-wheel for acceptable operating effort, add more or less tape as required for proper operation. 7. Reinstall barrel assembly. 8. Reinstall air outlet assembly into instrument panel.

For vehicles repaired under warranty use:

Labour Operation: D1440 Labour Time: 0.2 hr

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.