For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Power Mirror System Check? | -- | Go to Step 2 | Go to Outside Mirrors System Check
2 |

1. Disconnect the right power mirror connector.
2. Move the mirror select switch to the RIGHT position.
3. Connect a test lamp between the mirror switch connector terminal A and terminal C.
4. Operate the mirror switch to the UP position and the DOWN position.

Does the test lamp light in both positions?

--

Go to Step 3

Go to Step 5

3 |

1. Connect a test lamp between the mirror switch connector terminal C and terminal B.
2. Operate the mirror switch to the RIGHT position and the LEFT position.

Does the test lamp light in both positions?

--

Go to Step 4

Go to Step 6

4 | Replace the right mirror drive unit. Refer to Power Mirror Drive Replacement. Is the repair complete? | -- | Go to Outside Mirrors System Check | --
5 | Test the following circuits for an open:

• | CKT 1497

• | CKT 1498

Did you find an open in either of the circuits?

--

Go to Step 7

Go to Step 8

6 | Test the for an open in CKT 881. Did you find an open in CKT 881? | -- | Go to Outside Mirrors System Check | --
7 | Repair the open in the faulty circuit. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Outside Mirrors System Check | --
8 | Replace the outside mirror switch. Is the repair complete? | -- | Go to Outside Mirrors System Check | --