For 1990-2009 cars

## Instrument Panel Insulator Replacement Right

### Removal Procedure

1. Turn the retainer (2) to the instrument panel 1/4 turn.
2. Remove the courtesy lamp.
3. Remove the right sound insulator (3).

### Installation Procedure

1. Install the right sound insulator (3).
2. Install the courtesy lamp.
3. Turn the retainer (2) to the instrument panel 1/4 turn.

## Instrument Panel Insulator Replacement Left

### Removal Procedure

1. Turn the retainer (4) to the instrument panel 1/4 turn.
2. Remove the nut (3) from the accelerator pedal assembly.
3. Remove the courtesy lamp.
4. Remove the left sound insulator (2).

### Installation Procedure

1. Install the left sound insulator (2).
2. Install the courtesy lamp.
3. Install the nut (3) to the accelerator pedal assembly.
4. Turn the retainer (4) to the instrument panel 1/4 turn.