For 1990-2009 cars

## Front and Rear Side Door Center Molding Replacement Pontiac

### Removal Procedure

1. Remove the door center molding nuts (1).
2. Remove the door center molding screws (3).
3. Pull at the top of the door center molding (3) in order to disengage the molding from the clips (2).
4. For Pontiac GTs only, push down on the door center molding (6) in order to disengage the molding from the clips.
5. Remove the door center molding (6).

### Installation Procedure

1. Install the door center molding (6).
2. For Pontiac GTs only, engage the door center molding to the clips.
3. Push the door center molding (6) in order to engage the clips (2).
4. Install the door center molding screws (3).

## Front and Rear Side Door Center Molding Replacement Buick

### Removal Procedure

1. Remove the door center molding nuts (1).
2. Remove the door center molding screws (3).
3. Pull at the top of the door center molding (4) in order to disengage the molding from the clips (2).
4. Remove the door center molding (4).

### Installation Procedure

1. Install the door center molding (4).
2. Push the door center molding (4) in order to engage the clips (2)
3. Install the door center molding screws (3).