For 1990-2009 cars
Engine Controls Components
Engine Data Sensors
OBD II Symbol Description Notice
Engine Controls Connector End Views
Handling ESD Sensitive Parts Notice
Handling ESD Sensitive Parts Notice

### Circuit Description

The Powertrain Control Module (PCM) uses the manifold absolute pressure (MAP) sensor to control the fuel delivery and the ignition timing. The MAP sensor measures the changes in the intake manifold pressure which results from engine load, or intake manifold vacuum, and the RPM changes, and converts these into voltage outputs. The Powertrain Control Module (PCM) sends a 5 volt reference voltage to the MAP sensor. As the manifold pressure changes, the output voltage of the MAP sensor also changes. By monitoring the MAP sensor output voltage, the PCM knows the manifold pressure. A lower pressure, or low voltage, output voltage will be approximately 1.0 to 1.5 volts at idle. Higher pressures, or higher voltage, output voltage will be approximately 4.5 to 4.8 volts at wide open throttle (WOT). The MAP sensor is also used to measure barometric pressure, allowing the PCM to make adjustments for different altitudes.

### Conditions for Setting the DTC

• | DTC(s) P0122 or P0123 not set.

• | Engine has run for at least 20-40 seconds.

• | Throttle Position (TP) sensor is less than 12 %.

• | Vehicle speed is less than 1 mph (2 km/h).

• | MAP is greater than 82 kPa.

• | Above conditions met for 10 seconds.

### Action Taken When the DTC Sets

• | The Malfunction Indicator Lamp (MIL) will illuminate.

• | The Powertrain Control Module (PCM) will record operating conditions at the time the diagnostic fails. This information will be stored in the Freeze Frame and Failure Records buffers.

• | A history DTC is stored.

• | Coolant fan turns ON.

• | The PCM will substitute a fixed MAP value and use Throttle Position (TP) to control the fuel delivery (scan tool will not show defaulted value.)

• | The vehicle will operate in Open Loop when the vehicle is under 8 km/h (5 mph). The vehicle will operate in Closed Loop when the vehicle is over 8 km/h (5 mph).

### Conditions for Clearing the MIL/DTC

• | The MIL will turn OFF after three consecutive ignition cycles in which the diagnostic runs without a fault.

• | A history DTC will clear after 40 consecutive warm-up cycles without a fault.

• | The MIL/DTCs can be cleared by using the scan tool.

### Diagnostic Aids

With the ignition switch ON and the engine stopped, the manifold pressure is equal to atmospheric pressure and the signal voltage will be high.

This information is used by the PCM as an indication of vehicle altitude. Comparison of this reading with a known good vehicle with the same sensor is a good way to check the accuracy of a suspect sensor. Readings should be the same ± 0.4 volt.

If a DTC P0108 is intermittent, refer to Symptoms or to the Manifold Absolute Pressure Sensor Output Diagnosis for further diagnosis.

DTC P0108 may set as a result of misfire. If misfire is present, repair the cause of misfire before using this table. The misfire counters may be used to determine which cylinder(s) is misfiring.

Important: After repairs, use scan tool Fuel Trim Reset function to reset long term fuel trim to 128 (0%).

### Test Description

Number(s) below refer to the step number(s) on the Diagnostic Table.

1. The Powertrain OBD System Check prompts the technician to complete some basic checks and store the freeze frame and failure records data on the scan tool if applicable. This creates an electronic copy of the data taken when the fault occurred. The information is then stored in the scan tool for later reference.

2. This step will determine if DTC P0108 is the result of a hard malfunction or an intermittent condition.

3. This step simulates conditions for a DTC P0107. If the PCM recognizes the change, that indicates the PCM, the MAP sensor 5.0 volt reference circuit and the MAP sensor signal circuit are OK.

4. This step looks for an open MAP sensor ground circuit. If the circuit was open, additional DTCs will also be set. If no other DTC(s) are set and the circuit is found to be open, then the open must be between the MAP sensor and the electrical connector sensor ground splice.

5. When the MAP sensor signal circuit is shorted to battery voltage, the TP will be displayed above 0% at all times and A/C High Side will be displayed high. The vehicle will also remain in Open Loop.

6. The MAP sensor vacuum source should only supply vacuum to the MAP sensor. Check the vacuum port for a restriction caused by casting flash.

7. Disconnect all sensors that use a 5.0 volt reference one at a time while monitoring the short on the 5.0 volt reference circuit. Replace any sensor that may have caused the short on the 5.0 volt reference circuit.

8. Replacement PCMs must be reprogrammed and the crankshaft position system variation procedure must be performed. Refer to the latest Techline information for PCM programming and the Powertrain Control Module (PCM) for the Crankshaft Position System Variation Procedure .

#### DTC P0108-Manifold Absolute Pressure (MAP) Circuit-High Voltage

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Powertrain On-Board Diagnostic (OBD) System Check performed? | -- | Go to Step 2 | Go to Powertrain On Board Diagnostic (OBD) System Check
2 |

1. Install a scan tool.
2. With the engine idling.

Does the scan tool display a MAP voltage of the specified value or more?

4.0V

Go to Step 3

Go to Step 4

3 |

1. Turn the ignition switch OFF.
2. Disconnect the MAP sensor electrical connector.
3. Turn the ignition switch ON, with the engine OFF.

Does the scan tool display a MAP voltage of the specified value or less?

1.0V

Go to Step 5

Go to Step 6

4 |

1. Turn the ignition switch ON, with the engine OFF, review the Freeze Frame data and note the parameters.
2. Operate the vehicle within the freeze frame conditions and Conditions For Setting The DTC as noted.

Does the scan tool display a MAP voltage of the specified value or more?

4.0V

Go to Step 3

Go to Diagnostic Aids

5 | Connect a test light to battery voltage and probe the MAP sensor ground circuit. Does the test light illuminate? | -- | Go to Step 7 | Go to Step 11
6 | Check the MAP sensor signal circuit for a short to voltage and repair as necessary. Was a repair necessary? | -- | Go to Step 14 | Go to Step 12
7 | Connect a DVM to ground and probe the 5.0 volt reference circuit. Does the DVM display near the specified value or less? | 5V | Go to Step 8 | Go to Step 9
8 | Check the MAP sensor vacuum source for being plugged or leaking. Was a problem found? | -- | Go to Step 10 | Go to Step 13
9 | Check the 5.0 volt reference circuit for a short to voltage and repair as necessary. Was a repair necessary? | -- | Go to Step 14 | Go to Step 12
10 | Repair the vacuum source as necessary. Is the action complete? | -- | Go to Step 14 | --
11 | Check for an open or poor onnection in the MAP sensor ground circuit and repair as necessary Was a repair necessary? | -- | Go to Step 14 | Go to Step 12
12 | Replace the PCM. Is the action complete? | -- | Go to Step 14 | --
13 | Replace the MAP sensor. Is the action complete? | -- | Go to Step 14 | --
14 |

1. Using the scan tool, clear the DTCs.
2. Start the engine and idle at normal operating temperature.
3. Operate the vehicle within the conditions for setting this DTC as supported in the text.

Does the scan tool indicate that this diagnostic ran and passed?

--

Go to Step 15

Go to Step 2

15 | Check if any additional DTCs are set. Are any DTCs displayed that have not been diagnosed? | -- | Go to applicable DTC table | System OK