For 1990-2009 cars

### Removal Procedure

The relays in the illustration are described in the following order:

• | (1) A/C compressor clutch relay

• | (2) Fuel pump relay

• | (3) Cooling fan relay

• | (4) Blower motor relay

1. Remove the appropriate relay from the bracket.
2. Remove the electrical connector from the appropriate relay.

### Installation Procedure

The relays in the illustration are described in the following order:

• | (1) A/C compressor clutch relay

• | (2) Fuel pump relay

• | (3) Cooling fan relay

• | (4) Blower motor relay

1. Install the electrical connector to the appropriate relay.
2. Install the appropriate relay to the bracket