For 1990-2009 cars

## Inner Belt Sealing Strip Replacement Front

### Removal Procedure

1. Remove the door trim panel. Refer to Door Trim Panel Replacement .
2. Pull up in order to disengage the door inner belt sealing strip (1) from the door flange (2).

### Installation Procedure

1. Push down in order to engage the door inner belt sealing strip (1) to the door flange (2).
2. Install the door trim panel. Refer to Door Trim Panel Replacement .

## Inner Belt Sealing Strip Replacement Rear

### Removal Procedure

1. Remove the door trim panel. Refer to Door Trim Panel Replacement .
2. Pull up in order to disengage the door inner belt sealing strip (1) from the door flange.

### Installation Procedure

1. Push down in order to engage the door inner belt sealing strip (1) to the door flange.
2. Install the door trim panel. Refer to Door Trim Panel Replacement .