For 1990-2009 cars

## Door Frame Applique Replacement Front

### Removal Procedure

1. Lower the window to the full down position.
2. Remove the upper window run channel. Refer to Window Channel Replacement .
3. Remove the door applique screws (1).
4. Remove the door applique molding (2).

### Installation Procedure

1. Install the door applique molding (2).
2. Install the door applique screws (1).
3. Install the upper window run channel. Refer to Window Channel Replacement .

## Door Frame Applique Replacement Rear

### Removal Procedure

1. Lower the window to the full down position.
2. Remove the upper window run channel. Refer to Window Channel Replacement .
3. Remove the door applique screws (4).
4. Remove the door applique molding (5).

### Installation Procedure

1. Install the door applique molding (5).
2. Install the door applique screws (4).
3. Install the upper window run channel. Refer to Window Channel Replacement .