For 1990-2009 cars

### Removal Procedure

1. Remove the rear end spoiler nuts (3).
2. Disengage the spoiler tape (4). Use a vertical striking motion on one end of the spoiler assembly.
3. Remove the rear end spoiler retainers (2) from the deck lid.

### Installation Procedure

1. Install the rear spoiler retainers (4) to the rear end spoiler assembly (1).
2. Peel the backing paper from the spoiler tape.
3. Install the rear end spoiler assembly (1) to the vehicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the rear end spoiler nuts (3).

Tighten
Tighten the nuts to 4 N·m (35 lb in).