For 1990-2009 cars

### Removal Procedure

1. Remove the washer solvent from the container.
2. Remove the wheelhouse panel. Refer to Wheelhouse Panel Replacement .
3. Disconnect the electrical connector and the washer hose from the washer pump.
4. Remove the washer pump from the container.

### Installation Procedure

Important: The washer pump must be pushed completely into the container seal.

1. Install the washer pump into the solvent container.
2. Install the washer hose and the electrical connector.
3. Install the wheelhouse panel. Refer to Wheelhouse Panel Replacement .
4. Fill the solvent container with washer solvent.