For 1990-2009 cars

### Removal Procedure

Caution: When working with any type of glass or sheet metal with exposed or rough edges, wear approved safety glasses and gloves in order to reduce the chance of personal injury.

1. Unsnap the mirror housing.
2. Remove the mirror (2) and the plastic backing (1).

### Installation Procedure

1. Install the insulator on the rear of the plastic mirror backing (1).
2. Snap the mirror housing, install the mirror (2) and the plastic backing.