For 1990-2009 cars

### Removal Procedure

1. Remove cluster trim plate screws.
2. Remove the cluster trim plate.
3. Disconnect the electrical connectors.
4. Remove the cluster screws.
5. Disconnect the electrical connectors.
6. Twist the socket to remove.

### Installation Procedure

1. Push bulb into the socket.
2. Install the socket.
3. Connect the electrical connectors.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install cluster screws.

Tighten
Tighten the cluster screws to 2 N·m (17 lb in).

5. Connect the electrical connectors.
6. Install the cluster trim plate screws.

Tighten
Tighten the cluster trim plate screws to 2 N·m (17 lb in).