For 1990-2009 cars

The EBCM contains sophisticated on-board diagnostics. When a Scan Tool accesses the EBCM on-board diagnostics, the EBCM on-board diagnostics identify the source of any system malfunction as specifically as possible. The EBCM on-board diagnostics also diagnose whether the malfunction is intermittent. There are 3 VES Diagnostic Trouble Codes (DTCs) that assist with diagnostics. Refer to the Diagnostic System Check in Antilock Brakes for VES DTC diagnosis.

The following actions occur when using the Scan Tool:

• | The Scan Tool specifically identifies the last DTC.

• | The specific data stores at the time of the malfunction.

• | Information about the first five DTCs set and the last DTC set becomes available.

• | The input and output can be monitored.

• | Malfunction confirmation and repair verification are enabled.