For 1990-2009 cars

# LABOR OPERATION FOR SUNVISOR WIRING (INFORMATION)

#### SUBJECT: LABOR OPERATION FOR SUNVISOR WIRING AND/OR CONNECTOR REPAIR (INFORMATION)

#### MODELS: 1994-96 BUICK SKYLARK 1994-96 CHEVROLET BERETTA, CAVALIER, CORSICA 1994-96 OLDSMOBILE ACHIEVA 1994 PONTIAC SUNBIRD 1994-96 PONTIAC GRAND AM 1995-96 PONTIAC SUNFIRE

FOR A SUNVISOR WIRING AND/OR CONNECTOR REPAIR, USE LABOR OPERATION NUMBER N6487 FOR THE RIGHT SIDE OR N6488 FOR THE LEFT SIDE. LABOR TIME WILL BE 0.1 - 0.5 HRS.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.