For 1990-2009 cars

## Reverse Servo Replacement L82

### Removal Procedure

• |
- Disconnect the negative battery cable. Refer to

  Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

  in General Information.

• |
- Remove the EGR pipe from the exhaust manifold.

• |
- Remove the exhaust crossover pipe. Refer to 3100 (VIN M) Exhaust Crossover Pipe in Exhaust.

• |
- Depress the servo cover.

• |
- Remove the snap ring and the servo cover.

• |
- Remove the following parts:

• | The piston assembly

• | The sealing ring

• | The servo spring

• |
- For the disassembly of the servo piston assembly, refer to Reverse Servo Disassemble .

### Installation Procedure

1. Install the following parts:

• | The servo spring

• | The sealing ring

• | The piston assembly

2. Install the servo cover and the snap ring.
3. Install the exhaust crossover pipe. Refer to 3100 (VIN M) Exhaust Crossover Pipe in Exhaust.
4. Install the EGR pipe to the exhaust manifold.
5. Connect the negative battery cable.