For 1990-2009 cars

1. Use a small screwdriver in order to disconnect the wiring harness assembly (224) from the electrical connector (35) in the case.
2. Use a small screwdriver in order to disconnect the wiring harness assembly at the following locations:

• | The 1-2 and 3-4 shift solenoid valve (315)

• | The 2-3 shift solenoid valve (315)

• | The TCC PWM solenoid valve (325)

• | The TCC apply solenoid valve (315)

• | The TFT sensor (391) located on the case cover or on the spacer plate

• | The wiring harness clip

3. Remove the wiring harness assembly (224).