For 1990-2009 cars

# SERVICE MANUAL UPDATE-SEC. 0B MAINT/LUBE-TIRE PRESSURE SPEC.

#### SUBJECT: TIRE PRESSURE SPECIFICATIONS

#### MODELS/YEARS: 1992-93 ACHIEVA

An error exists in 1992-93 Achieva Service Manuals under Tire Pressure Specifications. Following are the corrected Tire Pressure Specifications.

Spare.................................. 415 kPa (60 PSI) P185/75Rl4............................. 240 kPa (35 PSI) P205/55Rl6 (RPO QLG)................... 240 kPa (35 PSI) P205/55R16 (RPO QMS)................... 210 kPa (30 PSI) All others............................. 210 kPa (30 PSI)

Please mark a reference to this bulletin on the last page of Section OB in the affected service manuals.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.