For 1990-2009 cars

### Disassembly Procedure

#### Tools Required

• | J 22227-A Bearing Remover

• | J 41677 Pilot

• | J 22912-01 Split Plate

1. Remove the front bearing using the J 22227-A and the J 41677 and a hydraulic press.
2. Remove the rear bearing and the 3rd/4th gear using the J 22912-01 inverted and a hydraulic press.
3. Remove the following items as an assembly using a hydraulic press:

• | The needle bearing

• | The collar

• | The 2nd gear

• | The 1st/2nd gear synchronizer

• | The 1st gear

• | The key

4. Remove the thrust bearing.
5. Remove the thrust bearing washer.